(footprint "USB-C power-only" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp d83a44fd-e29f-4ee6-8c8b-6829700ac977)
  )
  (fp_text value "USB-C power-only" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 513daf13-b4c2-410f-a726-f2aabc4c10ab)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 29fafdef-7a9d-403a-b037-6082339125ce)
  )
  (fp_rect (start -4.5 -3.25) (end 4.5 3.25)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.SilkS") (tstamp 9c346c8f-1eec-4b45-bff0-5b55d10da8f4))
  (pad "1" thru_hole oval (at 1.85 3.25) (size 1.1 0.7) (drill oval 0.7 0.3) (layers "*.Cu" "*.Mask") (tstamp d6c13631-0b73-46c1-9c06-77b31c92831b))
  (pad "2" thru_hole oval (at -1.85 3.25) (size 1.1 0.7) (drill oval 0.7 0.3) (layers "*.Cu" "*.Mask") (tstamp 12a0509b-83d4-497a-a614-5e58af2c19be))
  (pad "3" thru_hole oval (at -4.5 -0.7) (size 0.7 1.4) (drill oval 0.3 1) (layers "*.Cu" "*.Mask") (tstamp c3f107b9-cb4d-4a0e-ade4-3b6b006013a7))
  (pad "3" thru_hole oval (at 4.5 -0.7) (size 0.7 1.4) (drill oval 0.3 1) (layers "*.Cu" "*.Mask") (tstamp db265c48-406b-47a5-a482-a25ebda4b17e))
)
